To test this COECommDevice, use the CMIT tool in this folder to send/received COE messages. Both nodes must be using the same COE XML files to send/receive COE messages.

Configure CMIT tool as server since COECommDevice will configure itself as client by default(whether using TCP or UDP)

This COE instrument also calls into lower level COE code from Raytheon.Common library.  Read the COE code from there if interested to know how it works.